MAKİNE BİLGİLERİ
==================================================

Makine Adı    : Complete nonwoven plant, from fibers to no-woven fabric, with double card
Marka         : ..
Model         : 
Makine No     : MCH-000157
Durum         : 

--------------------------------------------------
AÇIKLAMA
--------------------------------------------------

Complete nonwoven plant, from fibers to no-woven fabric, with double card Full description of no-woven plant: - Fiber suction system that goes directly to the fiber opening device brand Dell&rsquo; Orco and Villani. Usually, it&rsquo;s able to process 25 quintals of blended in about 2.5 hours - Lubrication system entirely in stainless steel, with air pump and air / oil nebulization system and renewed electrical panel. - No. 2 preparation chambers, with automatic diverters / exchangers, both OMMI brand. One chamber average is enough to supply material for about 1-2 days (with fine products they easily can supply material for 2 days each chamber). The chambers can be used also for some blended fibers effects, like m&eacute;lange NB: the days of duration refer to an 8-hour shift - Pneumatic transport system of fibers from the chambers to the carding line. - Fiber feeding device for the carding machine, where the fibers arrive from preparation. Equipped with a fiber suction device for sampling, to work without going through preparation. Adjustable speed, has 2 photocells for filling (one of the two is safety) - No. 2 Bonino cards, with a 2-meter diameter drum, 8 couples of cylinders each (therefore 16 cylinders per drum), useful working width 2,800 mm Inlet compactor and compactor before the second carding machine, with scale (equipped with no. 4 load cells) to manage the speed based on weight. Spare fillet for the first card Edge recovery at the exit from the second carding machine, where the fiber ribbon is cut to make it uniform. - Cross lapper, maximum speed around 60/70 meters/minute, maximum working width 4 meters. PVC tapes with button, 3 inverter motors and air clutch for reversal. Variable speeds. - MALIMO MALIVLIES loom, current gauge 18, (works on average with gauges from 14 to 22) Edge recovery at the exit of the loom - MALIMO MALIWAT loom, with heated bars to be able to go faster. Current average speed 1200/1300 beat/minute, Current gauge 14 (works on average with gauges from 7 to 22) - Oil cooling system. - Cutter is available for both looms.