MAKİNE BİLGİLERİ
==================================================

Makine Adı    : Latex coating system from Brückner
Marka         : BRUECKNER
Model         : 
Yıl           : End of 1980
Makine No     : MCH-000197
Durum         : 

--------------------------------------------------
AÇIKLAMA
--------------------------------------------------

Latex coating system from Br&uuml;ckner&nbsp;Carpet coating and laminating systemTechnical data:Max. working width: 5200 mmThe closing machine can utilise all reserves.Can be used up to a span width of 5250 mm.Min. working width: 3400 mm for Prage 3500 mmDrive speed: 2 - 15 m/min.Drive: DC motorsOperating side: rightColour of the system: RAL 1.015 structureGoods transport system: vertical needle chainLength of one field: 3 mFans per field: 2Fan power: 7.5 kWHeating systems - per field: 2, separately above and below the bridgeAdjustable air temperature: 50 - 250 &deg;CAchievable temperature spread:160 &deg; above, 100 &deg; belowor 200 &deg; above, 125 &deg; belowSize of the dryerPre-drying: 5 fieldsGelation channel: 3 fieldsVulcanisation channel: 12 fieldsProduction speed: 9 m/min. with the following data:Primer: 725 g/m&sup2; dry, 76% dry matterFoam: 650 g/m&sup2; dry, 72% dry matterCarpet pile: 100% PAWeight of pile and backing: 600 g/m&sup2;Air temperature:Back 170&ndash;180 &deg;CFields 14 + 15 140 &deg;CPile side 135 &deg;CCooling: 50 &deg;C on the foam surface at 20 &deg;C room temperatureHeating time to _180/135 &deg;C: &bull; max. 20 min.Gas consumption during dryingDry goods: approx. 2.2.10 6 kcal/hincl. I-radiatorat 5 m working widthapprox. 200 kg/h gasat 5 m working widthapprox. 200 kg/h gasElectrical power of the channelsRecirculating air: Pre-drying approx. 62 kWGelling and vulcanisation channelapprox. 185 kWCooling fields approx. 40 kWHeated: Direct gasGas type: Propane or butane with 500 mm WS pressure in the distribution pipeInstalled heat output: 3 Gcal/hcorresponds to approx. 300 kg gas/h