MAKİNE BİLGİLERİ
==================================================

Makine Adı    : COMERIO ERCOLE calender n. 4 cylinders working width 2900 mm
Marka         : COMERIO ERCOLE
Model         : 
Yıl           : 1990
Makine No     : MCH-000172
Durum         : 

--------------------------------------------------
AÇIKLAMA
--------------------------------------------------

COMERIO ERCOLE calender n. 4 cylinders working width 2900 mm - Manufacturer: COMERIO ERCOLE - Model: 4-cylinder - Year of manufacture: 1990 (estimated) - Completely overhauled in year: 2008 - Cylinder width: 3.000 mm - Useful working width: 2.900 mm - Pendulum centering device with n. 3 cylinders - Metal detector - N. 2 dancer cylinders with adjustable tension at both entry and exit - Fabric infeed controlled by inverter - Maximum pressure: 50 tons - Fabric infeed with a fixed curved stretching cylinder and a spreading device - N. 4 cylinders: 2 chromed steel cylinders on the outside, heated with thermal oil, and 2 wool paper cylinders on the inside. N.B. The cylinder layout can be changed as needed. - the 4 cylinders can also be driven together via a chain so that all four rotate. This operation is typically performed to calender non-woven fabrics by regulating their thickness. - N. 1 new spare paper/wool cylinder. - Large tangential roll output motorized by inverter. - Forced cylinder lubrication. - Supplied with gas-fired boiler for heating the thermal oil dedicated to the calender, 80,000 kcal.